**ASSIGNMENT 4**

|  |  |
| --- | --- |
| Student name | Usman.H |
| Student register no | 421219106304 |
| Team id | PNT2022TMID38891 |
| Project name | IOT based safety gadget for child safety monitoring and notification |

Question:

Write code and connections in wokwi for the ultrasonic sensor

Whenever the distance is less than 100cms send an “alert” to the IBM cloud and display in the device recent events

Upload document with wokwi share link and images of IBM cloud

**Code:**

#include <WiFi.h>//library for wifi

#include <PubSubClient.h>//library for MQtt

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength);

//-------credentials of IBM Accounts------

#define ORG "9nv26m"//IBM ORG1"//DevANITION ID

#define DEVICE\_TYPE "Usman"// Device type mentioned in ibm watson IOT Platform

#define DEVICE\_ID "1234"//Device ID mentioned in ibm watson IOT Platform

#define TOKEN "12345678"     //Token

String data3;

float dist;

//-------- Customise the above values --------

char server[] = ORG ".messaging.internetofthings.ibmcloud.com";// Server Name

char publishTopic[] = "iot-2/evt/Data/fmt/json";// topic name and type of event perform and format in which data to be send

char subscribetopic[] = "iot-2/cmd/test/fmt/String";// cmd  REPRESENT command type AND COMMAND IS TEST OF FORMAT STRING

char authMethod[] = "use-token-auth";// authentication method

char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;//client id

//-----------------------------------------

WiFiClient wifiClient; // creating the instance for wificlient

PubSubClient client(server, 1883, callback ,wifiClient); //calling the predefined client id by passing parameter like server id,portand wificredential

int LED = 4;

int trig = 5;

int echo = 18;

void setup()

{

**Serial**.begin(115200);

pinMode(trig,OUTPUT);

pinMode(echo,INPUT);

pinMode(LED, OUTPUT);

delay(10);

wificonnect();

mqttconnect();

}

void loop()// Recursive Function

{

 digitalWrite(trig,LOW);

  digitalWrite(trig,HIGH);

  delayMicroseconds(10);

  digitalWrite(trig,LOW);

  float dur = pulseIn(echo,HIGH);

  float dist = (dur \* 0.0343)/2;

**Serial**.print ("Distancein cm");

**Serial**.println(dist);

  PublishData(dist);

  delay(1000);

  if (!client.loop()) {

    mqttconnect();

  }

}

/\*.....................................retrieving to Cloud...............................\*/

void PublishData(float dist) {

  mqttconnect();//function call for connecting to ibm

  /\*

     creating the String in in form JSon to update the data to ibm cloud

  \*/

  String object;

  if (dist <100)

  {

    digitalWrite(LED,HIGH);

**Serial**.println("object is near");

    object = "Near";

  }

  else

  {

    digitalWrite(LED,LOW);

**Serial**.println("no object found");

    object = "No";

  }

  String payload = "{\"distance\":";

  payload += dist;

  payload += "," "\"object\":\"";

  payload += object;

  payload += "\"}";

**Serial**.print("Sending payload: ");

**Serial**.println(payload);

  if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish ok");// if it sucessfully upload data on the cloud then it will print publish ok in Serial monitor or else it will print publish failed

  } else {

**Serial**.println("Publish failed");

  }

}

void mqttconnect() {

  if (!client.connected()) {

**Serial**.print("Reconnecting client to ");

**Serial**.println(server);

    while (!!!client.connect(clientId, authMethod, token)) {

**Serial**.print(".");

      delay(500);

    }

     initManagedDevice();

**Serial**.println();

  }

}

void wificonnect() //function defination for wificonnect

{

**Serial**.println();

**Serial**.print("Connecting to ");

  WiFi.begin("Wokwi-GUEST", "", 6);//passing the wifi credentials to establish the connection

  while (WiFi.status() != WL\_CONNECTED) {

    delay(500);

**Serial**.print(".");

  }

**Serial**.println("");

**Serial**.println("WiFi connected");

**Serial**.println("IP address: ");

**Serial**.println(WiFi.localIP());

}

void initManagedDevice() {

  if (client.subscribe(subscribetopic)) {

**Serial**.println((subscribetopic));

**Serial**.println("subscribe to cmd OK");

  } else {

**Serial**.println("subscribe to cmd FAILED");

  }

}

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength)

{

**Serial**.print("callback invoked for topic: ");

**Serial**.println(subscribetopic);

  for (int i = 0; i < payloadLength; i++) {

    //Serial.print((char)payload[i]);

    data3 += (char)payload[i];

  }

  //   Serial.println("data: "+ data3);

//   if(data3=="Near")

//   {

// Serial.println(data3);

// digitalWrite(LED,HIGH);

//   }

//   else

//   {

// Serial.println(data3);

// digitalWrite(LED,LOW);

//   }

data3="";

}

REFERENCE: https://wokwi.com/projects/349188561903288914



